\hypertarget{structmom__entrain__diffusive_1_1entrain__diffusive__cs}{}\doxysection{mom\+\_\+entrain\+\_\+diffusive\+::entrain\+\_\+diffusive\+\_\+cs Type Reference}
\label{structmom__entrain__diffusive_1_1entrain__diffusive__cs}\index{mom\_entrain\_diffusive::entrain\_diffusive\_cs@{mom\_entrain\_diffusive::entrain\_diffusive\_cs}}


\doxysubsection{Detailed Description}
The control structure holding parametes for the M\+O\+M\+\_\+entrain\+\_\+diffusive module. 

Definition at line 29 of file M\+O\+M\+\_\+entrain\+\_\+diffusive.\+F90.



Collaboration diagram for mom\+\_\+entrain\+\_\+diffusive\+::entrain\+\_\+diffusive\+\_\+cs\+:
\nopagebreak
\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=350pt]{structmom__entrain__diffusive_1_1entrain__diffusive__cs__coll__graph}
\end{center}
\end{figure}
\doxysubsection*{Public variables and constants}
\begin{DoxyCompactItemize}
\item 
\mbox{\Hypertarget{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a2f4439a404b0275605426ee86711d21a}\label{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a2f4439a404b0275605426ee86711d21a}} 
logical \mbox{\hyperlink{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a2f4439a404b0275605426ee86711d21a}{bulkmixedlayer}}
\begin{DoxyCompactList}\small\item\em If true, a refined bulk mixed layer is used with GVnk\+\_\+rho\+\_\+varies variable density mixed \& buffer layers. \end{DoxyCompactList}\item 
\mbox{\Hypertarget{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a29992ac06a99299cb1de98dd2f2b5ef2}\label{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a29992ac06a99299cb1de98dd2f2b5ef2}} 
integer \mbox{\hyperlink{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a29992ac06a99299cb1de98dd2f2b5ef2}{max\+\_\+ent\+\_\+it}}
\begin{DoxyCompactList}\small\item\em The maximum number of iterations that may be used to calculate the diapycnal entrainment. \end{DoxyCompactList}\item 
\mbox{\Hypertarget{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a494616228fc4770aebb8138359c1eb32}\label{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a494616228fc4770aebb8138359c1eb32}} 
real \mbox{\hyperlink{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a494616228fc4770aebb8138359c1eb32}{tolerance\+\_\+ent}}
\begin{DoxyCompactList}\small\item\em The tolerance with which to solve for entrainment values \mbox{[}H $\sim$$>$ m or kg m-\/2\mbox{]}. \end{DoxyCompactList}\item 
\mbox{\Hypertarget{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a1ab45176c75bd9dc5dda4f622360294f}\label{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a1ab45176c75bd9dc5dda4f622360294f}} 
real \mbox{\hyperlink{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a1ab45176c75bd9dc5dda4f622360294f}{rho\+\_\+sig\+\_\+off}}
\begin{DoxyCompactList}\small\item\em The offset between potential density and a sigma value \mbox{[}R $\sim$$>$ kg m-\/3\mbox{]}. \end{DoxyCompactList}\item 
\mbox{\Hypertarget{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a90befefd96d23e33df09235fd7eab51c}\label{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a90befefd96d23e33df09235fd7eab51c}} 
type(\mbox{\hyperlink{structmom__diag__mediator_1_1diag__ctrl}{diag\+\_\+ctrl}}), pointer \mbox{\hyperlink{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a90befefd96d23e33df09235fd7eab51c}{diag}} =$>$ N\+U\+LL()
\begin{DoxyCompactList}\small\item\em A structure that is used to regulate the timing of diagnostic output. \end{DoxyCompactList}\item 
\mbox{\Hypertarget{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a52e16663b95ee82411a1e7e784a3d229}\label{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a52e16663b95ee82411a1e7e784a3d229}} 
integer \mbox{\hyperlink{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a52e16663b95ee82411a1e7e784a3d229}{id\+\_\+kd}} = -\/1
\begin{DoxyCompactList}\small\item\em Diagnostic ID for diffusivity. \end{DoxyCompactList}\item 
\mbox{\Hypertarget{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a5c1079b55883f8af874f589555f836f3}\label{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a5c1079b55883f8af874f589555f836f3}} 
integer \mbox{\hyperlink{structmom__entrain__diffusive_1_1entrain__diffusive__cs_a5c1079b55883f8af874f589555f836f3}{id\+\_\+diff\+\_\+work}} = -\/1
\begin{DoxyCompactList}\small\item\em Diagnostic ID for mixing work. \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
The control structure holding parametes for the M\+O\+M\+\_\+entrain\+\_\+diffusive module. 

Definition at line 29 of file M\+O\+M\+\_\+entrain\+\_\+diffusive.\+F90.



The documentation for this type was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
/home/cermak/src/\+M\+O\+M6.\+devrob/src/parameterizations/vertical/M\+O\+M\+\_\+entrain\+\_\+diffusive.\+F90\end{DoxyCompactItemize}
